Brüel & Kjær - Noise Dose meter Link Software VP 7790  1.0    © 2000 by Brüel & Kjær

NOISE DOSEMETER SURVEY REPORT FORM

Report format	ISO Noise at Work Regulations
data filename	c:\b&k_app\fhlavt.dta

User entered information:

Company name	
Wearer's name	
Location	
Department	
Job function	
Payroll number	
Social Security number	

User entered notes:

Notes

Setup information:

Setup name	ISO85
Dosemeter model number	Brüel & Kjær-4443
Dosemeter serial number	000000
Frequency weighting for RMS	A
Frequency weighting for Peak	Linear
Time weighting	Fast
Measurement range	70 - 140  dB

User calibration information:

Instrument last checked on	15-06-2005	10:47:52
Microphone serial number	80000758228

Logging times:			Duration
	dd-mm-yyyy	hh:mm:ss	hh:mm:ss,ss
Start of run	06-10-2005	00:04:00
End of run	06-10-2005	00:06:00
Duration of run			00:02:00,00
Duration of pause			00:00:00,00

Results of measurements:

Sound exposure	0,00  Pa2hr
Sound exposure	11,64  Pa2sec
Daily personal exposure level Lep,d	60,0  dB
Equivalent sound level Leq	83,8  dB  Q = 3
Sound exposure level SEL	104,6  dB  No threshold; No criterion; Q = 3

Threshold level	75  dB	75  dB
Criterion level	85  dB	90  dB
Exchange rate Q	3	3
Actual measured dose	0,3194  %	0,101  %
8 Hour projected dose	76,653  %	24,24  %
Average sound level Lavg	83,8  dB	83,8  dB
Time weighted average level TWA	60,0  dB	60,0  dB
User specified projected period	08:00  hh:mm	08:00  hh:mm
User specified projected dose	76,653  %	24,24  %

Exceedance times:
	hh:mm:ss.ss	for % of run
Time under range	00:00:00,00	0,00  %
Above or equal to 70  dB	00:02:00,00	100,00  %
Above or equal to 85  dB	00:00:26,93	22,44  %
Above or equal to 90  dB	00:00:01,17	0,98  %
Above or equal to 100  dB	00:00:00,00	0,00  %
Above or equal to 115  dB	00:00:00,00	0,00  %
Above or equal to 140  dB	00:00:00,00	0,00  %
Time over range	00:00:00,00	0,00  %
Above or equal to user specified level	00:01:51,65	93,04  %
User specified level	80  dB

Maximum exceedance levels:
		at dd-mm-yyyy hh:mm:ss.ss
RMS maximum level (Fast)	93,0  dB	at  06-10-2005 00:04:03
Peak exceedance level	106,0  dB	at  06-10-2005 00:04:01

Statistical exeedance levels:

L10.0%	86,0  dB
L50.0%	83,0  dB
L90.0%	80,5  dB
L95.0%	79,5  dB
L99.0%	77,5  dB

Time history profiles:

Profiles	Off
Profile sample interval	n.a.
Profile function 1	n.a.
Profile function 2	n.a.